Controller Script
Interval = .6

[F1 HT +15]	send heat exchanger T every 15 sec
[*CTD]		clear the displays
[F2 DL 1]	set position 1
[F2 PI]		home (returns to position 1)
[*WPL]		wait for changes to finish
[*SS +]		begin collecting absorbance data
[*SW 260]	set 260 nm
[*D 100]	wait 1 min
[F1 CT +3]	automatically send sample holder T every 3 min
[F1 SS S 400]	set stirring to 400 rpm and turn it on
[F1 TT S 30]	set target to 30 C
[F1 TC +]	turn temperature control on
[*WT 1000 2]	wait for stable T (or 20 min)
[*MSG - Add DNA]
[*D 500]	wait 5 min for samples to re-equilibrate
[F1 CT -]	stop automatic sending of sample holder T
[F1 RR S 1.0]	set ramp rate to 1.00
[F1 TT S 90]	set target to 90 C (starts ramp)
[*CTD]		clear the displays
[*SS +]		changes button caption to Save Data
[*LS 125]	loop 125 times (about 62 min.)
   [F2 PL 1]	set to position 1
   [*D 5]	wait 0.05 min
   [F1 CT ?]	query current sample holder T
   [F2 PL 2]	set to position 2
   [*D 5]
   [F1 CT ?]
   [F2 PL 3]	set to position 3
   [*D 5]
   [F1 CT ?]
   [F2 PL 4]	set to position 4
   [*D 5]
   [F1 CT ?]
   [F2 PL 5]	set to position 5
   [*D 5]
   [F1 CT ?]
   [F2 PL 6]	set to position 6
   [*D 5]
   [F1 CT ?]
[*LE]		end of loop
[*MSG + The script is complete]
