Controller Script
Interval = .6 	(0.01 min)

[F1 HT +15]	send heat exchanger T every 15 sec
[*CTD]		clear the displays
[*SS +]		begin collecting absorbance data
[*SW 625]	set 260 nm
[*D 100]	wait 1 min
[F1 CT +3]	automatically send sample holder T every 3 min
[F2 PL 1]	set to position 1
[F2 PI]		home (and returns to position 1)
[*WPL]		wait for position change
[F1 SS S 1000]	set stirring to 1000 rpm and turn it on
[F1 TT S 20]	set target to 20 C
[F1 TC +]	turn temperature control on
[*WT 1000 2]	wait for stable T (or 20 min)
[F1 CT -]	stop automatic sending of sample holder T
[*SS +]		begin collecting absorbance data
		  (again, in case user stopped collection)
[*SZ]		auto zero (on lowest bleach conc)
[*D 100]	allow time to finish
[F2 PL 6]	set to position 6
[*MSG - Add dye (beginning with position 1).  Close lid.  Press Enter key.]
		waits for user to press Return
[*CTD]		clear the displays
[*SS +]		changes button caption to Save Data
[*LS 50]	loop 50 times (about 16 min.)
	[*LS 6]
		[*PL+]		move to next position
		[*WPL]		wait for position change
		[F1 CT ?]	get time point
				(by getting temperature)
	[*LE]		end of inner loop
[*LE]		end of outer loop
[*MSG + The script is complete]
